

| ITEM**NO.** | **DATE QUESTION RECEIVED** | **DATE QUESTION ANSWERED** | **QUESTION** | **GOVERNMENT RESPONSE** |
| --- | --- | --- | --- | --- |
|  | 6/18/2024 | 7/09/2024 | Regarding concrete patching the floor from through floor Plumbing demolition, may the method be tapcon into the underside of the existing floor, caulk perimeter then concrete patch from above? | Yes – we listed two acceptable methods, the method stated above and another system that can be filled from the floor the hole is on. |
|  | 6/18/2024 | 7/09/2024 | There are Shotcrete Specifications, please clarify where this work is on the Drawings. | No shotcrete is required. |
|  | 6/18/2024 | 7/09/2024 | Please provide load requirements, detail and exactly clarify where the temporary shoring is required for this project. | Temporary shoring is not required. Design accounts for existing conditions as provided in record documents. Should conditions vary upon construction, notify the EOR. |